# Summary

This assignment involved executing a series of AT commands to simulate sending and reading an SMS using the CelerSMS AT Emulator. While most steps executed as expected, two commands (`AT+CSQ?` and `AT+CMGR=1`) returned `ERROR`, indicating possible limitations in the emulator. Key observations:

- The modem responded to basic commands (`AT`, `AT+CSQ`, and `AT+CMGF=1`) as expected.

- SMS was successfully sent using `AT+CMGS`, and the modem responded with confirmation.

- `AT+CSQ?` and `AT+CMGR` returned errors; this may be due to emulator limitations. Workaround: use `AT+CSQ` instead of `AT+CSQ?`. SMS reading may not be supported in this emulator.